|  |
| --- |
| **UTC Project Information** |
| Project Title | MPC-487 – Investigation of Cross Laminated Timber Bridge Decks as a Sustainable Solution for Repair of Deficient Rural Wood Bridges |
| University | Colorado State University  |
| Principal Investigator | John W. van de Lindt |
| PI Contact Information | ProfessorDepartment of Civil and Environmental EngineeringColorado State UniversityPhone: (970) 491-6697Email: jwv@engr.colostate.edu |
| Funding Agencies | USDOT, Research and Innovative Technology Administration |
| Agency ID or Contract Number | DTRT13-G-UTC38 |
| Project Cost | $64,000 |
| Start and End Dates | September 30, 2013 to September 30, 2018 |
| Project Duration | September 30, 2013 to September 30, 2018 |
| Brief Description of Research Project | Wood bridge deck replacement using glue laminated timber panels has been investigated (see e.g. Moody et al, 1990) and shown to be effective. However, that body of research focuses on classical loading in bridge decks, namely vehicle loading, which is critical when considering bridge deck rehabilitation. The advent of cross laminated timber (CLT) in Europe and its introduction to North America brings with it the potential for application to bridge deck rehabilitation. CLT differs from traditional glue laminated timber in that each lamination layer is rotated 90 degrees to provide desirable mechanical properties in both directions. For bridges located in moderate seismic regions such as some locations within the mountain plains region the ability to resist and transfer in-plane shear in any directions is critical. Currently, no design procedure exists in North America for in-plane connections of CLT panels. |
| Describe Implementation of Research Outcomes (or why not implemented)Place Any Photos Here | Published in a journal paper for others to utilize the results as needed/desired. |
| Impacts/Benefits of Implementation(actual, not anticipated) | The results and method will allow for better modeling and validation of models for CLT bridge decks constructed/designed using CLT and subjected to lateral loads such as earthquakes. |
| Web Links* Reports
* Project Website
 | * [MPC Research Report](https://www.ugpti.org/resources/reports/details.php?id=1038)
* [CSU Thesis](https://mountainscholar.org/handle/10217/189259)
 |