|  |
| --- |
| UTC Project Information |
| Project Title | MPC-686 – Developing a Collision Warning and Collision Avoidance System for WYDOT Snowplows |
| University | University of Wyoming |
| Principal Investigator | Muhammad Tahmidul Haq, Ph.D., P.E.Suresh Muknahallipatna, Ph.D.Khaled Ksaibati, Ph.D., P.E. |
| PI Contact Information | Muhammad Tahmidul Haq, Ph.D., P.E.Postdoctoral Research AssociateWyoming Technology Transfer CenterUniversity of WyomingPhone: (307) 761-8078Email: mhaq@uwyo.eduORCID: 0000-0003-3307-288XSuresh Muknahallipatna, Ph.D.Professor and Graduate CoordinatorDept. of Electrical and Computer EngineeringUniversity of WyomingPhone: (307) 766-3174Email: sureshm@uwyo.eduORCID: 0000-0003-4153-524XKhaled Ksaibati, Ph.D., P.E.Professor and DirectorWyoming Technology Transfer CenterUniversity of WyomingPhone: (307) 766-6230Email: khaled@uwyo.eduORCID: 0000-0002-9241-1792 |
| Funding Source(s) and Amounts Provided (by each agency or organization) | USDOT, Office of the Assistant Secretary for Research and Technology$106,903Wyoming Department of Transportation$170,046 |
| Total Project Cost | $276,949 |
| Agency ID or Contract Number | 69A3551747108 |
| Start and End Dates | February 10, 2022 to July 31, 2023 |
| Brief Description of Research Project | This study aims at developing a rear-end collision warning and collision avoidance system for snowplow trucks and other maintenance vehicles to maximize the capability of preventing crashes and minimize the severity of crashes. To develop the system, the required number and type of sensors (e.g., rear-facing Lidar or Radar) will be developed and tested on the maintenance vehicles. The potential idea is to have technology that will activate if a vehicle enters within a designated distance behind the maintenance vehicle. Once a vehicle is within this designated area, the LED lights would become larger and brighter than the normal lights on the back. If this did not alert the trailing vehicle behind the maintenance vehicle and it continued to get closer, a warning light with a rear-facing air horn would sound to alert both vehicles. While receiving the warning signal, the plow operator could raise the plow to reduce the disturbance of the snow cloud. This action would allow the oncoming vehicle to see the plow and avoid a collision. In summary, the study seeks to provide a comprehensive information of benefits of using the proposed collision warning and collision avoidance system. |
| Describe Implementation of Research Outcomes (or why not implemented)Place Any Photos Here |  |
| Impacts/Benefits of Implementation(actual, not anticipated) |  |
| Web Links* Reports
* Project Website
 |  |